T5A 250V Radial 382 TR5 Fuse - Pack of 10

Description:

The T5A 382 TRS fuses come in a pack of 10 and have a voltage rating of 250V and 5A.

The 382 series of radial TR5 fuses have enhanced breaking capacity and are a slow blow / time-lag type fuse and designed in accordance with IEC 60127-3.

Specifications:

Rated Voltage: 250V

Rated Current: 5A

Type: Time Delay / Slow Blow

Case: Shock safe casing

Material:

Base/Cap: Brown Thermoplastic Polyamide

Round Pins: Copper, Tin-plated

Operating Temperature: -40 ~ +85°C

Dimensions: 8.5 mm x 8 mm

Lead Length: 18.8mm

Contents:

10 x T5A 250V Radial 382 TR5 Fuse

Amazon Keywords:

T5A 250V Radial 382 TR5 Fuse - Pack of 10

SKU: PHI1052357

UPC: 372278948781