**T5A 250V Radial 382 TR5 Fuse**

**Rated Voltage:** 250V

**Rated Current:** 5A

**Type:** Time Delay / Slow Blow

**Case:** Shock safe casing

**Material**:

Base/Cap: Brown Thermoplastic Polyamide

Round Pins: Copper, Tin-plated

**Operating Temperature:** -40 ~ +85°C

**Dimensions:** 8.5 mm x 8 mm

Lead Length: 18.8mm

 Long Leads (L=18.8mm)

 Short Leads (L=4.3mm)